Support OS:
Fedora Core 6 i386
Fedora Core 6 x86_64

Steps:
1. Use dd(Linux) or Rawritewin.exe(Windows) to write driver disk.
2. CD/DVD boot form OS installation disc.
3. Insert driver disk to floppy drive.
4. Add "linux dd" after "boot:" and press enter.
5. Select "YES" in "Do you have a driver disk?".
6. Select a device which you like to use.

Fixed bugs:
1. Driver recognizes JMB368 as JMB361.
2. JMB368 40/80 pins detection issue.

Known Issues:
None
