; This INF file installs the Silicon Image Serial ATA Raid driver
; for the SiI 3114 controller on systems using the 64-bit Intel
; Itainium processor.
;
; Copyright (C) 2003-2005 by Silicon Image, Inc.
; All rights reserved

[Version]
Signature="$Windows NT$"
Class=SCSIAdapter
ClassGuid={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%SI%
CatalogFile=SI3114r.cat
DriverVer=04/10/2006, 1.0.9.0


[SourceDisksNames.ia64]
1="Silicon Image SiI 3114 SATARaid Driver Installation Disk",Si3114r.inf,\ia64,

[SourceDisksFiles.ia64]
SI3114r.sys	= 1
SilSupp.cpl	= 1
SiWinAcc.sys	= 1


[DestinationDirs]
DefaultDestDir	= 12
DllFiles	= 11

[DriverFiles]
SI3114r.sys,,,0x20
SiWinAcc.sys,,,0x20

[DllFiles]
SilSupp.cpl,,,0x20

[Manufacturer]
%SI%=SI_HDC,NTia64

[SI_HDC.NTia64]
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_61141095
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_288510F1
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_81361043
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_81671043
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_047AA0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_0478A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_0479A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_90181695
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_F642270F
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_100415BD
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_12501462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_13101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_15601462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_16101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_B0031458
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1B711019
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_61141071
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_003515D4
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1025147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1001147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_130A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1C0A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_2A1E103C


[ControlFlags]
ExcludeFromSelect.ntx86=*



;; Driver install sections
;;
[SI_3114_XP.NTia64]
Copyfiles=DriverFiles, DllFiles

[SI_3114_XP.NTia64.Services]
AddService=SI3114r,0x00000002,SI_3114_Service_Install, Miniport_EventLog_Inst
AddService=SiFilter,,FilterService_Install

[SI_3114_XP.NTia64.CoInstallers]
Copyfiles=DllFiles
AddReg = SI_3114_CoInstall_AddReg

[SI_3114_CoInstall_AddReg]
HKR,,CoInstallers32,0x00010000,"SilSupp.cpl, CoInstHandler"


[SI_3114_Service_Install]
DisplayName=%SI3114.SvcDesc%
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\SI3114R.sys
LoadOrderGroup=Scsi miniport
AddReg=PnPSupport_AddReg
AddReg=ProblemDeviceList_AddReg
AddReg=SupportedSubSystemIds_AddReg


[FilterService_Install]
DisplayName=SATALink driver accelerator
ServiceType=1
StartType=0
ErrorControl=0
ServiceBinary=%12%\SiWinAcc.sys
LoadOrderGroup=Filter


; Mark device as supporting Plug & Play on the PCI(5) bus.
[PnPSupport_AddReg]
HKR,Parameters\PnPInterface,5,0x00010001,1


; List of devices with known configuration issues.
[ProblemDeviceList_AddReg]
HKR,ProblemDevices
HKR,ProblemDevices, %ProblemDev1Name%, 0, %ProblemDev1Value%


; List of controller subsystem IDs to be supported by the SI3114R.sys driver.
[SupportedSubSystemIds_AddReg]
HKR,SupportedSubsystemIDs,%PCI\VEN_1095&DEV_3114.DeviceDesc%,0x00010001, 0x61141095
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Fujitsu-Siemens 2885)",0x00010001, 0x288510F1
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Asus 8136)",0x00010001, 0x81361043
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Asus 8167)",0x00010001, 0x81671043
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 047A)",0x00010001, 0x047AA0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0478)",0x00010001, 0x0478A0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0479)",0x00010001, 0x0479A0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (EPoX 9018)",0x00010001, 0x90181695
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Chaintech F642)",0x00010001, 0xF642270F
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (DFI 1004)",0x00010001, 0x100415BD
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9125)",0x00010001, 0x12501462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9131)",0x00010001, 0x13101462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9156)",0x00010001, 0x15601462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9161)",0x00010001, 0x16101462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (GIGABYTE)",0x00010001, 0xB0031458
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ECS)",0x00010001, 0x1B711019
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MITAC)",0x00010001, 0x61141071
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (IWILL)",0x00010001, 0x003515D4
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit SC-1P)",0x00010001, 0x1025147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit WI-2P)",0x00010001, 0x1001147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x130A147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x1C0A147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (HP 2A1E)",0x00010001, 0x2A1E103C



;*************************************************************
;The NT EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,0x00010001,7


[Strings]
SI="Silicon Image"

PCI\VEN_1095&DEV_3114.DeviceDesc="Silicon Image SiI 3114 SATARaid Controller"
SI3114.SvcDesc="SiI-3114 SATARaid Controller"


ProblemDev1Name="Maxtor 4D060H3                          DAK05GK0"
ProblemDev1Value="MaxMode = UDMA-5"
