; This INF file installs the Silicon Image Serial ATA Raid driver
; for the SiI 3114 controller on systems running Windows 98/ME,
; Windows NT 4.0, Windows 2000/XP and Windows Server 2003.
;
; Copyright (C) 2003-2005 by Silicon Image, Inc.
; All rights reserved

[Version]
Signature="$Chicago$"
Class=SCSIAdapter
ClassGuid={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%SI%
;;CatalogFile=SI3114r.cat
DriverVer=11/02/2004, 1.0.0.8


[SourceDisksNames]
1="Silicon Image SiI 3114 SATARaid Driver Installation Disk",SI3114r.sys,,

[SourceDisksFiles]
SI3114r.sys	= 1
SiiSupp.vxd	= 1
SilSupp.cpl	= 1
SiWinAcc.sys	= 1

[DestinationDirs]
DefaultDestDir	= 12
DllFiles	= 11

[DriverFiles_9X]
SI3114r.mpd,SI3114r.sys,,0x20
SiiSupp.vxd,,,0x20

[DriverFiles_NT_2K]
SI3114r.sys,,,0x20

[DriverFiles_XP]
SI3114r.sys,,,0x20
SiWinAcc.sys,,,0x20

[DllFiles]
SilSupp.cpl,,,0x20

[Manufacturer]
%SI%=SI_HDC,NTx86.5.1

[SI_HDC]
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_61141095
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_288510F1
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_047AA0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_0478A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_0479A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_90181695
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_F642270F
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_100415BD
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_12501462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_13101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_15601462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_16101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_B0031458
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_1B711019
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_61141071
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_003515D4
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_1025147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_1001147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_130A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_1C0A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_81361043
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_2A1E103C

[SI_HDC.NTx86.5.1]
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_61141095
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_288510F1
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_047AA0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_0478A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_0479A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_90181695
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_F642270F
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_100415BD
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_12501462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_13101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_15601462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_16101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_B0031458
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1B711019
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_61141071
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_003515D4
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1025147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1001147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_130A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1C0A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_81361043
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_2A1E103C

;; Win9x install section
;;
[SI_3114]
Copyfiles=DriverFiles_9X, DllFiles
AddReg = ios, win98.reg, Win98ProblemDeviceList, Win98SupportedSubSystemIds


;; Windows NT4.0 and Windows 2000 install sections
;;
[SI_3114.NTX86]
Copyfiles=DriverFiles_NT_2K, DllFiles

[SI_3114.NTX86.Services]
AddService=SI3114r,0x00000002,SI_3114_Service_Install, Miniport_EventLog_Inst

[SI_3114.NTX86.CoInstallers]
AddReg = SI_3114_CoInstall_AddReg


;; Windows XP install sections
;;
[SI_3114_XP]
Copyfiles=DriverFiles_XP, DllFiles

[SI_3114_XP.Services]
AddService=SI3114r,0x00000002,SI_3114_Service_Install, Miniport_EventLog_Inst
AddService=SiFilter,0,FilterService_Install


[SI_3114_XP.CoInstallers]
AddReg = SI_3114_CoInstall_AddReg

[SI_3114_CoInstall_AddReg]
HKR,,CoInstallers32,0x00010000,"SilSupp.cpl, CoInstHandler"


[SI_3114_Service_Install]
DisplayName=%SI3114.SvcDesc%
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\SI3114R.sys
LoadOrderGroup=Scsi miniport
DelReg=NT4WorkAround_DelReg
AddReg=PnPSupport_AddReg
AddReg=PortConfigure_AddReg
AddReg=ProblemDeviceList_AddReg
AddReg=SupportedSubSystemIds_AddReg


[FilterService_Install]
DisplayName=SATALink driver accelerator
ServiceType=1
StartType=0
ErrorControl=0
ServiceBinary=%12%\SiWinAcc.sys
LoadOrderGroup=Filter


; Mark device as supporting Plug & Play on the PCI(5) bus.
[PnPSupport_AddReg]
HKR,Parameters\PnPInterface,5,0x00010001,1


[PortConfigure_AddReg]
HKR,Parameters\Device,NumberOfRequests,0x00010001, 64
HKR,Parameters\Device,MaximumSGList,0x00010001, 33


; List of devices with known configuration issues.
[ProblemDeviceList_AddReg]
HKR,ProblemDevices
HKR,ProblemDevices, %ProblemDev1Name%, 0, %ProblemDev1Value%


; Remove dummy registry value that may have been created during text mode
; setup of Windows NT4.0.  This value is created to work around the inability
; text mode setup to create multiple subkeys at a time.
[NT4WorkAround_DelReg]
HKR, Parameters, NT40WorkAround


; List of controller subsystem IDs to be supported by the SI3114R.sys driver on
; NT/Win2K/XP systems.

[SupportedSubSystemIds_AddReg]
HKR,SupportedSubsystemIDs,%PCI\VEN_1095&DEV_3114.DeviceDesc%,0x00010001, 0x61141095
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Fujitsu-Siemens 2885)",0x00010001, 0x288510F1
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 047A)",0x00010001, 0x047AA0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0478)",0x00010001, 0x0478A0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0479)",0x00010001, 0x0479A0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (EPoX 9018)",0x00010001, 0x90181695
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Chaintech F642)",0x00010001, 0xF642270F
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (DFI 1004)",0x00010001, 0x100415BD
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9125)",0x00010001, 0x12501462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9131)",0x00010001, 0x13101462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9156)",0x00010001, 0x15601462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9161)",0x00010001, 0x16101462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (GIGABYTE)",0x00010001, 0xB0031458
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ECS)",0x00010001, 0x1B711019
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MITAC)",0x00010001, 0x61141071
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (IWILL)",0x00010001, 0x003515D4
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit SC-1P)",0x00010001, 0x1025147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit WI-2P)",0x00010001, 0x1001147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x130A147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x1C0A147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ASUS P5GD/P5AD)",0x00010001, 0x81361043
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (HP 2A1E)",0x00010001, 0x2A1E103C

[Win98ProblemDeviceList]
HKLM,%Win98ProblemDeviceSubKey%
HKLM,%Win98ProblemDeviceSubKey%, %ProblemDev1Name%, 0, %ProblemDev1Value%


; List of controller subsystem IDs to be supported by the SI3114R.mpd driver on
; Windows 98/ME systems.
; NOTE: Because of a bug in the INF file handling on Win98, hex dword values that use letters A - F must be
;          specified as bytes, least significant byte first.
[Win98SupportedSubSystemIds]
HKLM, %Win98SupportedControllersSubKey%,%PCI\VEN_1095&DEV_3114.DeviceDesc%,0x00010001, 0x95,0x10,0x14,0x61
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Fujitsu-Siemens 2885)",0x00010001, 0xF1,0x10,0x85,0x28
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 047A)",0x00010001, 0xA0,0xA0,0x7A,0x04
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0478)",0x00010001, 0xA0,0xA0,0x78,0x04
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0479)",0x00010001, 0xA0,0xA0,0x79,0x04
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (EPoX 9018)",0x00010001, 0x95,0x16,0x18,0x90
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Chaintech F642)",0x00010001, 0x0F,0x27,0x42,0xF6
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (DFI 1004)",0x00010001, 0xBD,0x15,0x04,0x10
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI 9125)",0x00010001, 0x62,0x14,0x50,0x12
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI 9131)",0x00010001, 0x62,0x14,0x10,0x13
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI 9156)",0x00010001, 0x62,0x14,0x60,0x15
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI 9161)",0x00010001, 0x62,0x14,0x10,0x16
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (GIGABYTE)",0x00010001, 0x58,0x14,0x03,0xB0
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ECS)",0x00010001, 0x19,0x10,0x71,0x1B
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MITAC)",0x00010001, 0x71,0x10,0x14,0x61
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (IWILL)",0x00010001, 0xD4,0x15,0x35,0x00
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit SC-1P)",0x00010001, 0x7B,0x14,0x25,0x10
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit WI-2P)",0x00010001, 0x7B,0x14,0x01,0x10
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x7B,0x14,0x0A,0x13
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x7B,0x14,0x0A,0x1C
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ASUS P5GD/P5AD)",0x00010001, 0x43,0x10,0x36,0x81
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (HP 2A1E)",0x00010001, 0x3C,0x10,0x1E,0x2A



;*************************************************************
;The NT EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,0x00010001,7


[IOS]
HKR,,DevLoader,,*IOS
HKR,,DontLoadIfConflict,,"Y"


[WIN98.REG]
HKR,,PortDriver,,SI3114R.mpd


[Strings]
SI="Silicon Image"

PCI\VEN_1095&DEV_3114.DeviceDesc="Silicon Image SiI 3114 SATARaid Controller"
SI3114.SvcDesc="SiI-3114 SATARaid Controller"


Win98ProblemDeviceSubKey = "System\CurrentControlSet\Services\SI3114R\ProblemDevices"
Win98SupportedControllersSubKey = "System\CurrentControlSet\Services\SI3114R\SupportedSubsystemIDs"


ProblemDev1Name="Maxtor 4D060H3                          DAK05GK0"
ProblemDev1Value="MaxMode = UDMA-5"
