; This INF file installs the Silicon Image Serial ATA non-Raid driver
; for the SiI 3114 controller on systems using the 64-bit Intel
; Itainium processor.
;
; Copyright (C) 2003 -2006 by Silicon Image, Inc.
; All rights reserved

[Version]
Signature="$Windows NT$"
Class=SCSIAdapter
ClassGuid={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%SI%
CatalogFile=SI3114.cat
DriverVer=06/21/2006, 1.2.8.0


[SourceDisksNames.ia64]
1="Silicon Image SiI 3114 SATALink Driver Installation Disk",Si3114.inf,\ia64,

[SourceDisksFiles.ia64]
SI3114.sys	= 1
SilSupp.cpl	= 1
SiWinAcc.sys	= 1


[DestinationDirs]
DefaultDestDir	= 12
DllFiles		= 11


[DriverFiles]
SI3114.sys,,,0x20
SiWinAcc.sys,,,0x20

[DllFiles]
SilSupp.cpl,,,0x20


[Manufacturer]
%SI%=SI_HDC,NTia64

[SI_HDC.NTia64]
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_31141095
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_288610F1
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_31148086


[ControlFlags]
ExcludeFromSelect.ntx86=*



;; Driver install sections
;;
[SI_3114_XP.NTia64]
Copyfiles=DriverFiles, DllFiles

[SI_3114_XP.NTia64.Services]
AddService=SI3114,0x00000002,SI_3114_Service_Install, Miniport_EventLog_Inst
AddService=SiFilter,0,FilterService_Install

[SI_3114_XP.NTia64.CoInstallers]
Copyfiles=DllFiles
AddReg = SI_3114_CoInstall_AddReg


[SI_3114_CoInstall_AddReg]
HKR,,CoInstallers32,0x00010000,"SilSupp.cpl, CoInstHandler"


[SI_3114_Service_Install]
DisplayName=%SI3114.SvcDesc%
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\SI3114.sys
LoadOrderGroup=Scsi miniport
AddReg=PnPSupport_AddReg
AddReg=PortConfigure_AddReg
AddReg=ProblemDeviceList_AddReg
AddReg=SupportedSubSystemIds_AddReg


[FilterService_Install]
DisplayName=SATALink driver accelerator
ServiceType=1
StartType=0
ErrorControl=0
ServiceBinary=%12%\SiWinAcc.sys
LoadOrderGroup=Filter


; Mark device as supporting Plug & Play on the PCI(5) bus.
[PnPSupport_AddReg]
HKR,Parameters\PnPInterface,5,0x00010001,1


[PortConfigure_AddReg]
HKR,Parameters\Device,NumberOfRequests,0x00010001, 64
HKR,Parameters\Device,MaximumSGList,0x00010001, 33
HKR, Parameters\Device, CreateInitiatorLU, 0x00010001, 1


; List of devices with known configuration issues.
[ProblemDeviceList_AddReg]
HKR,ProblemDevices
HKR,ProblemDevices, %ProblemDev1Name%, 0, %ProblemDev1Value%


; List of controller subsystem IDs to be supported by the SI3114.sys driver.
[SupportedSubSystemIds_AddReg]
HKR,SupportedSubsystemIDs,%PCI\VEN_1095&DEV_3114.DeviceDesc%,0x00010001, 0x31141095
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Tyan)",0x00010001, 0x288610F1
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Intel)",0x00010001, 0x31148086


;*************************************************************
;The NT EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,0x00010001,7


[Strings]
SI="Silicon Image"

PCI\VEN_1095&DEV_3114.DeviceDesc="Silicon Image SiI 3114 SATALink Controller"
SI3114.SvcDesc="SiI-3114 SATALink Controller"


ProblemDev1Name="Maxtor 4D060H3                          DAK05GK0"
ProblemDev1Value="MaxMode = UDMA-5"
