; This INF file installs the Silicon Image Serial ATA Raid driver
; for the SiI 3114 controller on systems running Windows 98/ME,
; Windows NT 4.0, Windows 2000, and Windows XP.
;
; Copyright (C) 2003-2004 by Silicon Image, Inc.
; All rights reserved

[Version]
Signature="$Chicago$"
Class=SCSIAdapter
ClassGuid={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%SI%
CatalogFile=SI3114r.cat
DriverVer=02/03/2004, 1.0.0.7


[SourceDisksNames]
1="Silicon Image SiI 3114 SATARaid Driver Installation Disk",SI3114r.sys,,

[SourceDisksFiles]
SI3114r.sys	= 1
SiiSupp.vxd	= 1
SiWinAcc.sys	= 1

[DestinationDirs]
DefaultDestDir	= 12
DllFiles		= 11

[DriverFiles_9X]
SI3114r.mpd,SI3114r.sys,,0x20
SiiSupp.vxd,,,0x20

[DriverFiles_NT_2K]
SI3114r.sys,,,0x20

[DriverFiles_XP]
SI3114r.sys,,,0x20
SiWinAcc.sys,,,0x20


[Manufacturer]
%SI%=SI_HDC,NTx86.5.1

[SI_HDC]
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_61141095
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_288510F1
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_047AA0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_0478A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_0479A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_90181695
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_F642270F
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_100415BD
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_12501462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_13101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_15601462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_16101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_B0031458
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_1B711019
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_61141071
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_003515D4
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_1025147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_1001147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_130A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_1C0A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114, PCI\VEN_1095&DEV_3114&SUBSYS_81361043

[SI_HDC.NTx86.5.1]
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_61141095
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_288510F1
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_047AA0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_0478A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_0479A0A0
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_90181695
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_F642270F
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_100415BD
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_12501462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_13101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_15601462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_16101462
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_B0031458
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1B711019
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_61141071
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_003515D4
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1025147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1001147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_130A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_1C0A147B
%PCI\VEN_1095&DEV_3114.DeviceDesc%=SI_3114_XP, PCI\VEN_1095&DEV_3114&SUBSYS_81361043

;; Win9x install section
;;
[SI_3114]
DriverVer=02/03/2004, 1.0.0.7
Copyfiles=DriverFiles_9X, DllFiles
AddReg = ios, win98.reg, Win98ProblemDeviceList, Win98SupportedSubSystemIds


;; Windows NT4.0 and Windows 2000 install sections
;;
[SI_3114.NTX86]
Copyfiles=DriverFiles_NT_2K

[SI_3114.NTX86.Services]
AddService=SI3114r,0x00000002,SI_3114_Service_Install, Miniport_EventLog_Inst



;; Windows XP install sections
;;
[SI_3114_XP]
Copyfiles=DriverFiles_XP

[SI_3114_XP.Services]
AddService=SI3114r,0x00000002,SI_3114_Service_Install, Miniport_EventLog_Inst
AddService=SiFilter,,FilterService_Install




[SI_3114_Service_Install]
DisplayName=%SI3114.SvcDesc%
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\SI3114R.sys
LoadOrderGroup=Scsi miniport
AddReg=PnPSupport_AddReg
AddReg=ProblemDeviceList_AddReg
AddReg=SupportedSubSystemIds_AddReg


[FilterService_Install]
DisplayName=SATALink driver accelerator
ServiceType=1
StartType=0
ErrorControl=0
ServiceBinary=%12%\SiWinAcc.sys
LoadOrderGroup=Filter


; Mark device as supporting Plug & Play on the PCI(5) bus.
[PnPSupport_AddReg]
HKR,Parameters\PnPInterface,5,0x00010001,1


; List of devices with known configuration issues.
[ProblemDeviceList_AddReg]
HKR,ProblemDevices
HKR,ProblemDevices, %ProblemDev1Name%, 0, %ProblemDev1Value%


; List of controller subsystem IDs to be supported by the SI3114R.sys driver on
; NT/Win2K/XP systems.
[SupportedSubSystemIds_AddReg]
HKR,SupportedSubsystemIDs,%PCI\VEN_1095&DEV_3114.DeviceDesc%,0x00010001, 0x61141095
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Fujitsu-Siemens 2885)",0x00010001, 0x288510F1
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 047A)",0x00010001, 0x047AA0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0478)",0x00010001, 0x0478A0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0479)",0x00010001, 0x0479A0A0
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (EPoX 9018)",0x00010001, 0x90181695
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Chaintech F642)",0x00010001, 0xF642270F
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (DFI 1004)",0x00010001, 0x100415BD
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9125)",0x00010001, 0x12501462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9131)",0x00010001, 0x13101462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9156)",0x00010001, 0x15601462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI MS9161)",0x00010001, 0x16101462
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (GIGABYTE)",0x00010001, 0xB0031458
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ECS)",0x00010001, 0x1B711019
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MITAC)",0x00010001, 0x61141071
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (IWILL)",0x00010001, 0x003515D4
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit SC-1P)",0x00010001, 0x1025147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit WI-2P)",0x00010001, 0x1001147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x130A147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x1C0A147B
HKR,SupportedSubsystemIDs,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ASUS P5GD/P5AD)",0x00010001, 0x81361043

[Win98ProblemDeviceList]
HKLM,%Win98ProblemDeviceSubKey%
HKLM,%Win98ProblemDeviceSubKey%, %ProblemDev1Name%, 0, %ProblemDev1Value%


; List of controller subsystem IDs to be supported by the SI3114R.mpd driver on
; Windows 98/ME systems.
[Win98SupportedSubSystemIds]
HKLM, %Win98SupportedControllersSubKey%,%PCI\VEN_1095&DEV_3114.DeviceDesc%,0x00010001, 0x95,0x10,0x14,0x61
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Fujitsu-Siemens 2885)",0x00010001, 0xF1,0x10,0x85,0x28
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 047A)",0x00010001, 0xA0,0xA0,0x7A,0x04
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0478)",0x00010001, 0xA0,0xA0,0x78,0x04
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Aopen 0479)",0x00010001, 0xA0,0xA0,0x79,0x04
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (EPoX 9018)",0x00010001, 0x95,0x16,0x18,0x90
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Chaintech F642)",0x00010001, 0x0F,0x27,0x42,0xF6
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (DFI 1004)",0x00010001, 0xBD,0x15,0x04,0x10
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI 9125)",0x00010001, 0x62,0x14,0x50,0x12
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI 9131)",0x00010001, 0x62,0x14,0x10,0x13
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI 9156)",0x00010001, 0x62,0x14,0x60,0x15
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MSI 9161)",0x00010001, 0x62,0x14,0x10,0x16
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (GIGABYTE)",0x00010001, 0x58,0x14,0x03,0xB0
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ECS)",0x00010001, 0x19,0x10,0x71,0x1B
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (MITAC)",0x00010001, 0x71,0x10,0x14,0x61
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (IWILL)",0x00010001, 0xD4,0x15,0x35,0x00
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit SC-1P)",0x00010001, 0x7B,0x14,0x25,0x10
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit WI-2P)",0x00010001, 0x7B,0x14,0x01,0x10
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x7B,0x14,0x0A,0x13
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (Abit)",0x00010001, 0x7B,0x14,0x0A,0x1C
HKLM, %Win98SupportedControllersSubKey%,"%PCI\VEN_1095&DEV_3114.DeviceDesc% (ASUS P5GD/P5AD)",0x00010001, 0x43,0x10,0x36,0x81



;*************************************************************
;The NT EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,0x00010001,7


[IOS]
HKR,,DevLoader,,*IOS
HKR,,DontLoadIfConflict,,"Y"


[WIN98.REG]
HKR,,PortDriver,,SI3114R.mpd


[Strings]
SI="Silicon Image"

PCI\VEN_1095&DEV_3114.DeviceDesc="Silicon Image SiI 3114 SATARaid Controller"
SI3114.SvcDesc="SiI-3114 SATARaid Controller"


Win98ProblemDeviceSubKey = "System\CurrentControlSet\Services\SI3114R\ProblemDevices"
Win98SupportedControllersSubKey = "System\CurrentControlSet\Services\SI3114R\SupportedSubsystemIDs"


ProblemDev1Name="Maxtor 4D060H3                          DAK05GK0"
ProblemDev1Value="MaxMode = UDMA-5"
